
This configuration is for a HIFI playback device such as a DAC or amplifier, optimized for robustness and quality, not for latency.

The driver package has the following properties:

- USB streaming is set to ExtraSafe (32 ms)
- ASIO buffer size will be selected automatically by the driver
- No control panel is available. User cannot change settings manually.