XMOS driver information



This driver has been issued for the following product:

"ENGINEERED eR-xu2s"

Digital audio stereo playback interface board
for evaluation purpose, DIY'ers and OEM use.

PID: 0x3076
VID: 0x20B1

